****

**Figure**  TGA thermogram of Poly)St-co-GMA(. Copolymerization process included combining St and GMA with different feed monomer compositions, namely M1= 70/30, M2= 50/50, and M3 = 30/70.